
CLARIFICATIONS TO THE PROCUREMENT DOCUMENTS
Questions and Answers – 30 October 2026
Procurement: Services for the Installation, Maintenance and Dismantling of an Art Installation at the Justus Lipsius Building in Brussels
The following questions and answers are published for the information of all interested Suppliers.
Q1. How will the carpet be protected?
A: Wood is never placed directly on the carpet. A flame-resistant cushioning fabric, cut to size, goes directly under the logs; plastic sheeting is rolled out around the structure to keep the area clean. Logs are laid straight onto the fabric without dragging.
Q2. Is the bottom layer cut to fit once in place, or removable?
A: Not cut on site. Pre-cut pieces are placed under each section of the structure; the surrounding plastic is rolled out wider. Nothing is left behind on the carpet.
Q3. Are the bottom and surrounding layers the same material?
A: No. The under-layer is flame-resistant cushioning; the surrounding layer is plastic, for cleanliness only.
Q4. How is the correct position of each piece identified?
A: Every log has an engraved number that cannot wear off. Letters marking each side are written on the protective plastic, so pieces can be placed without consulting the plan.
Q5. For dismantling and reassembly in the foyer, will the artist be present or is there a manual?
A: Detailed written instructions with full numbering will be provided, based on the test assembly in Lithuania. The artist will attend if any doubts remain.
Q6. Do all pieces fit in the foyer?
A: Yes. This was checked; the project was designed starting from the foyer's dimensions.
Q7. Are special or metal connectors used for the roof beams, and is the roof built in place or assembled on the ground and raised?
A: Most likely assembled on the ground frame by frame and raised. Fixings may be small metal screws rather than wooden dowels. The height is reachable from a ladder; no machinery is needed and the parts are not heavy. Details will be confirmed after the test assembly (~2 weeks) and written into the instructions.
Q8. Will the charred wood leave black marks?
A: It is treated with one layer of wax impregnation, so it leaves minimal marks. Some dust residue is expected; it collects on the protective layer and can be vacuumed. Corners can be taped.
Q9. Can the charred logs break?
A: Not in half. Small fragments may come off, mainly after transport; charcoal may be brought for touch-ups.
